**Printing Glucose Sensor Adapter Platform in the Form 3B**

Refer to Formlabs best practices: <https://support.formlabs.com/s/article/Model-Orientation?language=en_US>

Additional Notes:

* Print the entire body at an angle of 45 degrees, with support for best result.
* After it finishes printing, let it sit for 20 minutes, to allow excess Resin to drain back into the tank. Note: keep the cover closed so no light enters and cures any leftover material.
* Remove Resin that remains in the cavity with a serialized tool or use a can of air with gentle pressure directed at cavity.
* After the bath; carefully remove model from build plate.